int ledred = "10";

int ledgreen = "11";

void setup()

{

pinMode(10, OUTPUT);

pinMode(11, OUTPUT);

Serial.begin(9600);

Serial.println("Input Red to Turn on 10 and Green to turn on 11 and Input 3 to Turn off 10 and Input 4 to Turn off 11 ");

}

void loop() {

if (Serial.available())

{

int state = Serial.parseInt();

if (state == 1)

{

pinMode(LED\_BUILTIN, HIGH);

Serial.println("Command completed LED turned ON");

}

if (state == 2)

{

pinMode(LED\_BUILTIN, LOW);

Serial.println("Command completed LED turned OFF");

}

}

}

Sir I failed I am sure